PC-Dmis 2010 MR2 Object Library | Send comments on this topic. | See Object Hierarchy Chart
OPTIONPROBE Object Members
See Also Overview

Collapse All Expand All

# Public Properties

LowForce | Read/Write: Low force setting Double value used to set or get the probe low force setting.
ManFineProbing | Read/Write: Man Fine Probing
MaxForce | Read/Write: Maximum force setting Double value used to set or get the probe max force setting.
PositionalAccuracy | Read/Write: Positional Accuracy Double value used to set or get the positional accuracy setting.
ProbeAccuracy | Read/Write: Probe Accuracy setting Double value used to set or get the probe accuracy setting.
ProbingMode | Read/Write: Probing Mode
ReturnData | Read/Write: Return data setting Double value used to set or get the probe return data value.
ReturnSpeed | Read/Write: Return speed setting Double value used to set or get the probe return data value.
ScanAcceleration | Read/Write: Scan Acceleration
ScanOffsetForce | Read/Write: Scan Offset Force
ScanPointDensity | Read/Write: Scan Point Density Double value used to set or get the probe scan point density setting.
TriggerForce | Read/Write: Trigger force setting Double value used to set or get the probe scan point density setting.
UpperForce | Read/Write: Upper force setting Double value used to set or get the probe upper force setting.

# See Also

OPTIONPROBE Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.