## Creating Generic Loops

Looping Parameters dialog box

The Insert | Flow Control Command | Looping menu option allows you to repeat the part program (or portions of the part program) with or without any of the offsets. The LOOP command can be added anywhere in the part program, although this function is most useful at the beginning and end of the program.

More:

Uses for Looping

End Number

Start Number

Skip Number

Axes and Angle Offset

Loop Ids

Variable ID

End Loop