### MLB-113 Negative probe diameter invalidated calibration

A probe calibration operation resulted in computing a negative probe diameter. This is typically caused by specifying the wrong size for the calibration sphere or having the wrong measurement units active when specifying the calibration sphere size.

Effect

Command is not executed.

What you should do

1. Correct the problem and recalibrate the probe.