### Constructing a Cast Point

A point can be constructed by changing any given feature into the point. PC-DMIS will construct the point at the centroid of the input feature.

To construct a Cast Point:

1. Access the Construct Point dialog box (Insert | Feature | Constructed | Point).

2. Select the Cast option from the list of options.

3. Select any feature.

4. Click the Create button.

The Edit window command line for this option would read:
CONSTR/POINT,CAST,feat_1

Constructing a Cast Point from a Circle