### Constructing a Projected Line

A line can be constructed from any feature and a plane. PC-DMIS will project the line where the plane intersects the line. If there is only one input feature, the projection will be to the work plane.

To construct a Projected Line:

1. Access the Construct Line dialog box (Insert | Feature | Constructed | Line).

2. Select the Projection option.

3. Select either one or two features. The first feature may be of any type. If two features are selected, the second feature must be a plane.

4. Click the Create button.

Command line in the Edit window:
CONSTR/LINE,PROJ,feat_1,(feat_2),
length

Constructing a Line from a Line and a Plane | A - Constructed Line projected from the a line feature (LIN1) onto a plane feature (PLN1).