Current Help System: PC-DMIS CMM (View Core Help)

#### Touch Speed

The Touch Speed box allows you to specify the touch speed for the PH9 calibration.

To change the touch speed:

1. Select the existing value.

2. Enter a new value. This value should be a percent between 1% and 100%, with 1 being the slowest and 100 the fastest.

See "Touch Speed %" in the "Setting your Preferences" section in the PC-DMIS Core documentation for additional information.

Note: The number in the Touch Speed box can contain no more than four decimal places. If a number with more than four decimal places is entered, PC-DMIS rounds the number off at the fourth decimal place.