Current Help System: Direct CAD Interfaces (View Core Help)

## Unigraphics Direct CAD Interface

Follow the procedures in this section to install PC-DMIS and configure your system to use the Unigraphics Direct CAD Interface.

- Make sure you have full administrator rights before proceeding.

- If you haven't already done so, install Unigraphics V15 or higher on the same computer that will run PC-DMIS. You may use either a floating (network) license or locked license to run the Unigraphics DCI. However, you must be able to run Unigraphics on the local machine in order for PC-DMIS to be able to interface with Unigraphics You must have, at minimum, the Unigraphics gateway and ufunc_execute options; if not, you can purchase them from Unigraphics (see http://www.unigraphics.com). For NX 5 and higher, you will also need the solid_modeling and assemblies Unigraphics features.

More:

Step 1: Installing PC-DMIS

Step 2: Test the Unigraphics Direct CAD Interface