Current Help System: PC-DMIS Portable (View Core Help)

### Measuring Circle and Slot Features with Reflectors

When you measure a hole or a internal slot with a reflector attached to a pin nest probe, be sure to lift the probe away from the center of the internal feature when you finish creating or measuring the feature. This way PC-DMIS will properly calculate the vectors. Otherwise the feature's vector may be reversed.