Current Help System: PC-DMIS Settings Editor (View Core Help)

### Use Trax With SP600

The default 3D calibration algorithm for the SP600 has been changed to Trax. Of course you are free to try out which algorithm works best for your particular situation.

If using Trax calibration for the SP600, the effective tip size generated from the calibration will differ from the design value.

If using Trax calibration for non-SP600 analog probes on the Wetzlar machines, the design value of the tip size is used because tip size deviation is handled differently.

If using non-Trax calibration, the design value of the tip size is used.

Entry Name: UseTraxWithSP600

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is -1.