Current Help System: PC-DMIS Settings Editor (View Core Help)

### Focus Hi Accuracy

When this value is set to TRUE, the Vision machine will perform a second, slightly slower, pass-to attempt to improve the accuracy of the focal position. The second pass is optimized based on the image data of the first pass. This provides the default setting for the associated Vision Auto Feature target.

Entry Name: FocusHiAccuracy

Entry Type: True/False value. Default value is FALSE.