Current Help System: PC-DMIS Settings Editor (View Core Help)

### Scan Dialog Dir Tech1

This option determines the first technique that will be used for your advanced scan. Available options are Line, Body Axis, Variable and Nullfilter. Using Line (0) technique, the approach of the probe is perpendicular to the line between the previous two hits. Using Body Axis (1) technique, the approach of the probe is perpendicular to the indicated axis (see ScanDialogBodyAxis). Using Variable (2) technique, the approach of the probe is perpendicular to the line between the previous two hits but additional calculations are made using the min/max increments and angles to determine increments between hits. Using Nulfilter (3) technique, data is not filtered.

Entry Name: ScanDialogDirTech1

Entry Type: Whole Number specifying technique number. Default value is 0.