Current Help System: PC-DMIS Settings Editor (View Core Help)

### Iterate And RePierce Cad On Best Fit Alignments Max Loops

This value is used in conjunction with the "IterateAndRePierceCadOnBestFitAlignments" when that value is set to TRUE. This number sets the maximum number of loops that will be used for the alignment process. Limiting the number of loops is needed in case the alignment never converges to a solution.

Entry Name: IterateAndRePierceCadOnBestFitAlignmentsMaxLoops

Entry Type: Whole Number to specify number of loops. Default value is 100.

Administrator permission is required to change entry