Current Help System: PC-DMIS Settings Editor (View Core Help)

### Renishaw Calibration Use Additional Scans SP25

With the updated Renishaw calibration DLL added to PC-DMIS version 4.3 some of the scans that were required with the older CALRSP.DLL are now optional. Omitting the additional scans should not cause any significant reduction in accuracy. When set to 0, PC-DMIS will omit the scans for the SP25 probe, saving time during calibration. Set this value to 1, If for any reason there is a desire/need to include these additional scans.

Entry Name: RenishawCalibrationUseAdditionalScansSP25

Entry Type: Whole Number to specify using additional scans for an SP25 probe. Default value is 0.