Current Help System: PC-DMIS Settings Editor (View Core Help)

### Triangle Or Outline

When this value is set to 1 (Outline), the symbolic triangle for the plane will be sized so that its vertices are exactly where the measured points are. This value is used for Laser probes while the "DccPlnDisplay" value is used for Contact probes.

Entry Name: TriangleOrOutline

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.