Current Help System: PC-DMIS Settings Editor (View Core Help)

### Smallest Tip Search Increment In Degrees

Determines the conical tolerance for added tip changes. This allows PC-DMIS to utilize a tip that has a shank vector that is within the tolerance of the optimal vector angle for a given feature. For features such as points, lines, and planes there is a built in conical range of 90 degrees since a plane with a vector of 0, 0, 1 could be measured by t1a0b0 or t1a90b0. In the case of these features, PC-DMIS adds the user entered value to the built-in range. The proposed tip angle is also checked by running collision detection (silently) to determine if the tip will actually work.

Entry Name: SmallestTipSearchIncrementInDegrees

Entry Type: Real Number to specify angle in MM. Default value is 5.