Current Help System: PC-DMIS Vision (View Core Help)

#### Capture Button

The Capture button collects actual measured data as the nominals for a feature. To use the capture button:

1. Place the NC-100 video probe over the feature to be measured.

2. Set up parameters for the video probe by clicking the Video Setup button.

3. When finished, click the Capture button.

PC-DMIS, along with the NC-100 computer system will measure the feature and place the measured data in the THEO boxes. This allows you to measure features without CAD data.