Current Help System: PC-DMIS Vision (View Core Help)

### Cad View

Sample Cad View showing the Vision probe's field of view

The Cad View is the standard view of the part and works the same way as in the standard PC-DMIS software. For in depth information on the Cad View, see "The Graphics Display Window" topic in the "Navigating the Interface" section of the main PC-DMIS help file.

The green rectangular region shown in the CAD view is the "field of view" (FOV). The FOV represents the view through the video camera. The center of the field of view has a cross hair. On a machine supporting DCC motion, you can click and drag this crosshair to move the FOV to a new location on the part:

Moving the FOV

On a machine supporting DCC optics changing, you can also resize (magnify or shrink) the FOV by dragging the corners of the green box. This will change the current magnification:

Sizing the FOV