PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
Calibration Object Members
See Also Overview

Collapse All Expand All

# Public Properties

Moved | Read/Write: Indicates whether tool has been moved since it was calibrated Determines whether or not the sphere used as the calibration tool has moved since the last tip calibration.
SphereID | Read/Write: ID of sphere used for calibration This returns or sets the ID of a sphere command that occurs prior to the calibration command. The sphere should have identical characteristics with the tool identified by ToolID.
ToolID | Read/Write: ID of Tool of same dimensions as reference sphere Returns or sets the ID of a previously defined calibration tool that is similar to the sphere identified by SphereID. The tool data is used in the tip calibration or reset depending on the value of the moved data member.

# See Also

Calibration Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.