PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
DimensionCmd Object Members
See Also Overview

Collapse All Expand All

# Public Methods

AddAxes | Add default location axes for End Location command
Evaluate | Evaluates the dimension Evaluates a dimension’s data from its feature data.

# Public Properties

Angle | Read/Write: Angle value for angularity dimensions Represents the theoretical angle of a DIMENSION_ANGULARITY dimension.
ArrowMultiplier | Read/Write: Returns/Sets arrow multiplier Multiplier for display arrows of dimension.
AXIS | Read/Write: Returns/Sets axis value Axis used with dimension. Possible values include the following: DIMAXIS_NONE DIMAXIS_XAXIS DIMAXIS_YAXIS

DIMAXIS_ZAXIS

AxisLetter | Read Only: Dimension axis letter used to identify dimension type Axis letter used to describe the axis or type of the dimension.
Bonus | Read Only: Bonus value for position dimensions Returns the bonus tolerance of a true position dimension.
Datum1 | Read/Write: First datum feature
Datum1Modifier | Read/Write: First datum material condition
DATUM2 | Read/Write: Second datum feature
Datum2Modifier | Read/Write: Second datum material condition
Datum3 | Read/Write: Third datum feature
Datum3Modifier | Read/Write: Third datum material condition
DevAngle | Read Only: Deviation Angle Value Returns the deviation angle of a dimension.
Deviation | Read Only: Deviation Value Returns the deviation of a dimension.
DimensionModifier | Read/Write: Dimension material condition
Feat1 | Read/Write: First Reference feature/datum Returns the ID of the first feature associated with a dimension.
Feat2 | Read/Write: Second Reference feature/datum Returns the ID of the second feature associated with a dimension.
Feat3 | Read/Write: Third Reference feature/datum Returns the ID of the second feature associated with a dimension.
GraphicalAnalysis | Read/Write: Returns/Sets graphical analysis value Flag indicating whether graphical analysis is ON for the dimension.
ID | Read/Write: Dimesion ID Returns the ID of a dimension.
IsLocationAxis | Read Only: Returns the setting used to identify if the axis belongs to a Location Dimension Determines whether or not the axis is a Location axis.
IsTruePosAxis | Read Only: Returns the setting used to identify if the axis belongs to a Position Dimension Determines whether or not the axis is a Location axis.
Length | Read/Write: Reference Length Value Returns the length associated with a dimension.
Max | Read Only: Dimension Max Value Returns the maximum value of a dimension.
Measured | Read Only: Dimension Measured Value Returns the measured value of a dimension.
Min | Read Only: Dimension Min Value Returns the minimum value of a dimension.
Minus | Read/Write: Minus Tolerance Value Represents the negative tolerance of a dimension.
NOMINAL | Read/Write: Dimension Nominal Value Returns the nominal associated with a dimension.
OutputMode | Read/Write: Returns/Sets dimension output mode Output mode of the dimension. Possible values include the following: DIMOUTPUT_STATS DIMOUTPUT_REPORT

DIMOUTPUT_BOTH

OutTol | Read Only: Out of Tolerance Value Returns the out-of-tolerance value of a dimension.
ParallelPerpendicular | Read/Write: Parallel/Perpendicular value for 2d Dimensions Indicates whether calculations are performed parallel or perpendicular to input for 2-D dimensions. Possible values include the following: DIM_PERPINDICULAR DIM_PARALLEL
Parent | Read Only: Returns Parent Command Object
Plus | Read/Write: Plus Tolerance Value Returns the positive tolerance of a dimension. Read-only Double.
Profile | Read/Write: Form/Location Setting for Profile Dimensions This represents an enumerated value indicating what type of profile should be used. Possible values include the following: DIM_PROF_FORM_ONLY DIM_PROF_FORM_AND_LOCATION
RadiusType | Read/Write: Radius Setting for Position Dimensions Radius calculation type used with true position dimensions. Possible values include the following: DIM_NO_RADIUS DIM_ADD_RADIUS DIM_SUB_RADIUS
TextualAnalysis | Read/Write: Returns/Sets textual analysis value Flag indicating whether textual analysis is ON for the dimension.
TruePositionDatumModifier | Read/Write: Position material condition
TruePositionModifier | Read/Write: Position modifier Enumeration value indicating material conditions that should be used to calculate possible bonus tolerances. Possible values include the following: DIM_RFS_RFS DIM_RFS_MMC DIM_RFS_LMC

DIM_MMC_RFS

DIM_MMC_MMC

DIM_MMC_LMC

DIM_LMC_RFS

DIM_LMC_MMC

DIM_LMC_LMC

TruePosUseAxis | Read/Write: Use Axis setting for Position Dimensions Enumeration value indicating axis type to use with true position dimension. Possible values include the following: DIM_AXIS_AVERAGE DIM_AXIS_START_POINT

DIM_AXIS_END_POINT

Units | Read/Write: Dimension Units Unit type in use by dimension. Possible values include the following: INCH MM (for millimeters)

# See Also

DimensionCmd Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.