PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
ControlPoint Object
See Also Members

Collapse All Expand All

# Description

With the ControlPoint object you can insert control point locations. These locations interrupt the normal scan and alter scan speed, point density or both for defined portions of the scan.

# Remarks

The ControlPoint object is used with only the following scans:

- LinearOpen
- LinearClose
- Patch
- Section
- Line (Basic Scan)

Additionally, the ControlPoint object only works on machines that use an analog probe that allows continuous contact scanning.

In the PC-DMIS documentation, the Control Points are called Interrupt Points. See "Interrupts" in the "Scanning Your Part" section of your PC-DMIS documentation.

# See Also

ControlPoint Members

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.