PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
BSBOUNDCOND_ENUM Enumeration
See Also

Collapse All Expand All

# Members

Member | Value | Description
--- | --- | ---
BSBOUNDCOND_SPHERE | 600010 | Represents a Spherical Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, Diameter, number of Crossings.
BSBOUNDCOND_PLANECROSS | 600030 | Represents a Planar Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionPlaneV, number of Crossings.
BSBOUNDCOND_CYLINDER | 600040 | Represents a Cylindrical Boundary Condition. This Boundary condition requires the following parameters to be set by you using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionAxisV, Diameter, number of Crossings.
BSBOUNDCOND_CONE | 600050 | Represents a Conical Boundary Condition. This Boundary condition requires the following parameters to be set you user using Automation Properties and/or Automation Methods : BoundaryConditionCenter, BoundaryConditionEndApproach, BoundaryConditionAxisV, HalfAngle, number of Crossings.

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.