PC-Dmis 2010 MR3 Object Library | Send comments on this topic. | See Object Hierarchy Chart
MasterSlaveDlg Object Members
See Also Overview

Collapse All Expand All

# Public Methods

Calibrate | Runs the Master/Slave calibration process.

# Public Properties

Application | This read-only object returns the Application object.
DCC | Gets or sets whether the Master / Slave calibration is a manual (0) or DCC (1) calibration.
MasterProbe | Gets or sets which probe is used on the Master machine. The names are taken from the owning PartProgram object's Probes collection.
MasterTip | Gets or sets which tip is used on the Master machine. The names are taken from the owning PartProgram object's Probes collection.
MeasuringArm | Gets or sets which arm or arms measure the calibration sphere.
Parent | This read-only object returns the parent Application object.
Position | Gets or sets the first (or only) sphere position.
SlaveProbe | Gets or sets which probe is used on the Slave machine. The names are taken from the owning PartProgram object's Probes collection.
SlaveTip | Gets or sets which tip is used on the Slave machine. The names are taken from the owning PartProgram object's Probes collection.
tool | Gets or sets which calibration tool is being measured during the calibration process. The names are taken from the owning PartProgram object's Tools collection.
Visible | Determines whether or not the Master / Slave dialog box is visible.

# See Also

MasterSlaveDlg Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.