### MP-047 Temperature Compensation D/A failure

A D/A conversion on the Temperature Compensation board failed to complete within the allotted time of 32 milliseconds.

What you should do

1. To clear the error, click Clear error in the XYZ Display window. To clear it using an RCU-II, press and hold down the Servo Power Off button and then press the Joy button twice.

2. If the error reoccurs, call your Giddings & Lewis service representative.