#### To Create New Marked Sets

1. Select the Edit | Markings | New Marked Set option or double-click anywhere in the Marked Sets window, the New Mark Set dialog box appears requesting a name for the new marked set.

New Mark Set dialog box

2. Type a name to identify the marked set. While there's no limit to the length of the name, short descriptive keywords improve readability.

3. Click OK. Your new marked set is stored in the Marked Sets window. At this point PC-DMIS also displays a Report Print Options dialog box. This dialog box allows you to define printing options specific to this marked set. (See "Setting Output and Printer Options" in "Using Basic File Options" for information on the various options in this dialog box.)

A Sample Report Print Options dialog box for Set1

2. Define specific printing options for this set. Or, if you want to use the existing print options defined for your entire part program, simply select the Use Global Print Settings check mark.

3. Click OK. The dialog box closes.

4. You will now need to access the newly Marked Set and add features to it. Follow the procedure in the "To Add Features to Existing Marked Sets" topic to accomplish this.