### Execute Feature

To execute only the feature on which the cursor rests, select the File | Partial Execution | Execute Feature option.

PC-DMIS will display the Execution Mode Options dialog box. If PC-DMIS is set to manual mode (mode = MANUAL), it will prompt you to take the necessary hits. If PC-DMIS is set to DCC mode (mode = DCC), it will automatically move the probe based on the parameters set in the dialog box.

To maintain good execution speeds, PC-DMIS will not generate a report in the Report window if using the Execute Feature functionality. However, you can still view report-like information inside the Status Window.