Current Help System: PC-DMIS CMM (View Core Help)

### Circle Analog Scan Strategy

Description

This strategy performs a single circle scan around an internal or external circular feature.

1. From the Measurement Strategies tab, choose Circle Analog Scan Strategy. The Probe Toolbox tabs will change to only show Contact Path Properties and Contact Auto Move Properties.

2. Set the options in the Probe Toolbox and the other options in the Auto Feature dialog box as needed.

3. Click Properties. Modify the strategy's properties as needed. See "Available Measurement Strategy Properties".

4. Click Create.

- The scan moves according to the Direction defined in Measurement properties area of the Auto Feature dialog box.

- Once the scan finishes, PC-DMIS sets the strategy back to the default.

Adjustable Properties

See "Available Measurement Strategy Properties" for information on the available properties.