Current Help System: PC-DMIS CMM (View Core Help)

#### Reset Tips to Theo at Start of Calibration

If you mark this check box, the tip(s) undergoing calibration will automatically be reset back to their original theoretical conditions when the calibration starts. This essentially functions the same as if you manually clicked the Reset Tips button in the Probe Utilities dialog box before calibration.

This functionality does not apply to all types of operations and/or all types of hardware however. For example, it does not affect a "Qualification Check" operation because that is only a test of the calibration and does not actually change any calibration related data. It also does not apply when using infinite wrist devices in a mapped mode.

Its main purpose is to be used with the “Calibrate Tips” operation when used with a fixed head, indexing wrist, or infinite wrist if used in an indexing (non-mapped) mode.