Current Help System: Direct CAD Interfaces (View Core Help)

## Unigraphics Direct CAD Interface

Follow the procedures in this section to install PC-DMIS and configure your system to use the Unigraphics Direct CAD Interface.

- Make sure you have full administrator rights before proceeding.

- If you haven't already done so, install Unigraphics V15 or higher on the same computer that will run PC-DMIS. You may use either a floating (network) license or locked license to run the Unigraphics DCI. However, you must be able to run Unigraphics on the local machine in order for PC-DMIS to be able to interface with Unigraphics

- You must have, at minimum, the Unigraphics gateway.

- For versions NX 1 through NX 4 you will also need the ufunc_execute license feature.

- For NX 5 and higher, you DO NOT need the ufunc_execute license feature, but you will need the solid_modeling and assemblies license features.

- The Planner DCI requires the gateway, solid_modeling, assemblies, and drafting license features.

You can purchase any needed license features from Unigraphics (see http://www.unigraphics.com).

More:

Step 1: Installing PC-DMIS

Step 2: Test the Unigraphics Direct CAD Interface