Current Help System: PC-DMIS Laser (View Core Help)

### COP Command Mode Text

The COP command inside the Edit window’s Command Mode looks like this:

COP1 =COP/DATA,SIZE=0
REF,,

The COP command must precede any scan referring to it in the part program.

For example the example of REF,SCN2 shown below points to the SCN2 scan and will use its data:

COP2 =COP/DATA,SIZE=0
REF,SCN2,,

You can have more than one scan refer to a COP command.