Current Help System: PC-DMIS Laser (View Core Help)

#### Feature Based Clipping Parameters

PC-DMIS can clip laser data in both horizontal and vertical directions by typing a distance in the Horizontal box and, where available, the Vertical box. This distance will clip all the laser data outside of the defined distance excluding that data when extracting the feature.

While all the features support horizontal clipping, only these Auto Features support vertical clipping:

- Circle

- Polygon

- Edge Point

- Round Slot

- Square Slot

- Surface Point

- Plane

The clipping distances defined in the Feature Based clipping rings are shown as colored rings. The horizontal clipping appears as a yellow ring and the vertical clipping as a light-green ring.

Sample Circle Auto Feature with Horizontal Clipping (A) and Vertical Clipping Ring (B)