Current Help System: PC-DMIS Laser (View Core Help)

#### Point Cloud

This parameter defines the COP command from which the auto feature will be extracted. If "disabled" is selected, then the data from the scan will be stored internally by PC-DMIS. You can delete internal data if needed by using the Operation | Laser Autofeatures submenu. See "Clearing Auto Feature Scan Data".

Note: The "disabled" option is only used with DCC laser scans.