Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Optics Cal Pixel Size Verify Step Factor

This defines the fraction of the total number of zoom calibration magnification steps used for the verification steps. For example, if there are 25 calibration steps and the value is set to 0.3, the verification step will be 25 * 0.3 = 7. The smaller the value, the more zoom portions PC-DMIS will verify.

Entry Name: ProbeQualVisionOpticsCalPixelSizeVerifyStepFactor

Entry Type: Real Number specifying the fraction of the total number of zoom calibration magnification steps. The default is 0.3.