Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Tessellation Multiply Value

Represents the Multiplier Value for probe CAD tessellation. PC-DMIS multiplies the Multiplier Value by the tessellation value for the given CAD system. These values are then used in the generation of the shaded image. See the "TessellationMultiplyValue" for non-probe tessellation.

Entry Name: ProbeTessellationMultiplyValue

Entry Type: Real Number to specify Multiplier value. Default value is 1.