Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Zones

Stores the default Zones value that is used in the Measure Vision Probe dialog box. A larger number will create more sample zones around the angle range. Systems using higher magnification optics may find it better to use more zones and a smaller "ProbeQualVisionZonesCoveragePercent" value to better sample the angle range in a reasonable amount of time.

Entry Name: ProbeQualVisionZones

Entry Type: Whole Number specifying number of zones. The default is 8.