Current Help System: PC-DMIS Settings Editor (View Core Help)

### Stable Probing Time Delay

This provides the time delay value after which a stable probing hit will be triggered if Stable Probing mode is used within the PC-DMIS Portable software. This will only trigger a hit if the probing distance exceeds the value specified in the StableProbingDistance entry.

Entry Name: StableProbingTimeDelay

Entry Type: Real Number to specify time delay in seconds. Default value is 3.