Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Clearance Plane

Allows you to define the default value for the Clearance Plane option that will be used when an Auto Feature is created. When this option is set to TRUE (1), a `MOVE/CLEARPLANE` command is inserted before the feature being created. The Probe will move beyond the defined clearance plane before it measures the feature.

Entry Name: AutoClearancePlane

Entry Type: Whole Number to specify TRUE (1) or FALSE(0). Default value is 0.