Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Thickness Distance

Specifies the thickness of a plastic or sheet metal part where the CAD data only describes one side. PC-DMIS applies this material thickness automatically when using the CAD surface data. This thickness will be applied automatically along the surface normal vector each time CAD data is selected. Positive or negative values can be used.

Entry Name: DccThicknessDistance

Entry Type: Real Number to specify thickness. Default value is 0.