Current Help System: PC-DMIS Settings Editor (View Core Help)

### Command Identification - ID Letters

The Starting Letters value determines the first letter(s) that will be used in the identification process. PC-DMIS will always display the ID using capital letters. Up to 15 characters can be typed in.

Entry Name: (A,C,COPOper,CS,D,FCF,F,L,Q,V)Ltrs(0-17)

Entry Type: Character String to specify starting letters. Default value varies.

Note: Preferably this value should be set from the ID Setup tab of the SetUp Options (F5) dialog box within PC-DMIS.

Command Key:

ALtrs0 | Alignments
CLtrs0 | Comments
COPOperLtrs0 | Pointcloud Operator
CSLtrs0 | Call Subs
DLtrs(0-16) | Dimension/Angle - Symmetry
FCFLtrs(0-16) | Feature Control Frame
FLtrs(0-17) | Feature/Blobs - Surfaces
LLtrs0 | Label
QLtrs0 | SPC Queries
VLtrs0 | Variables

See Also:

Command Identification - ID Length

Command Identification - ID Starting Number