#### Stop

The Stop command button halts the probe at its current position and suspends execution of the part program.

Note: This option will not stop the part program execution if the current move is a PH9 orientation change. The program will stop after the PH9 has stopped.

The topic "Manually Controlling a Feature's Measurement" discusses using Stop to switch to manual mode during the execution process.