### MP-083 Laser not stable after warm-up time limit

The laser tube has not warmed up within the allowable time.

What you should do

1. To clear the error, power the MP down.

2. Power the MP back up.

3. If the error reoccurs, take off the covers and check the status lights at the back of each laser to determine which laser is at fault.

4. If the error persists, call your Giddings & Lewis service representative.