### Using the Execution Mode Options Dialog Box

All execution operations begin by displaying the Execution Mode Options dialog box.

Execution Mode Options dialog box

PC-DMIS will then execute all marked commands of the current part program.

- If you are in Manual Mode, PC-DMIS will request you to take hits.

- If you are in DCC Mode, PC-DMIS will automatically begin the measurement process.

More:

Machine Errors

Machine Commands

Continue

Stop

Erase Hit

Skip

Step-Next

Jump

Progress Bar

Manually Controlling a Feature's Measurement

Re-sizing the Execution Mode Options Dialog Box