### Johansson Interface

The Johansson interface is used with Johansson machines. This interface requires Proto software that is installed as part of the JoWin installation. When PC-DMIS starts it will also start the Proto software and terminate Proto when you exit PC-DMIS. Proto detects the communication setting to communicate with the controller.

Before starting PC-DMIS, rename the johansson.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Johansson interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).