Current Help System: PC-DMIS CMM (View Core Help)

### Cylinder Spiral Scan Strategy

Description

This strategy performs a spiral scan along the cylinder.

1. From the Measurement Strategies tab, choose Cylinder Spiral Scan Strategy. The Probe Toolbox tabs will change to only show Contact Path Properties and Contact Auto Move Properties.

2. Set the options in the Probe Toolbox and the other options in the Auto Feature dialog box as needed.

3. Click Properties. Modify the strategy's properties as needed. See "Available Measurement Strategy Properties".

4. Click Create.

- The scan moves according to the Direction defined in Measurement properties area of the Auto Feature dialog box.

- Once the scan finishes, PC-DMIS sets the strategy back to the default.

Adjustable Properties

See "Available Measurement Strategy Properties" for information on the available properties.