Current Help System: Direct CAD Interfaces (View Core Help)

### Using the OrbixPort Entry

I-DEAS uses a software product called Orbix as an information broker between applications over a network. PC-DMIS uses Orbix™ to send and receive information from the I-DEAS server. By default, I-DEAS uses TCP/IP port 1570 for Orbix communications across a network. If I-DEAS does not use the default port, then you need to specify the port using the OrbixPort entry in the PC-DMIS Settings Editor.

This port value is located in the [Ideas] section of the Settings Editor. See "Setting Advanced Registry Options: Introduction" for information on changing Settings Editor values.

More:

To Determine the Orbix Port