Current Help System: Direct CAD Interfaces (View Core Help)

#### Modify the Registry

1. Open the Settings Editor.

2. Click on the plus sign (+) next to the CATIA section. The list expands.

3. Modify the CatiaPort, CatiaAddress, and CatiaDirectory entries so that they contain the IP address of the CATIA UNIX workstation, a valid port number, and the directory location of the CATIA files to import. See "Example of the Registry Modified with CATIA Information:".

4. Save and close the Settings Editor when you are finished modifying it.