Current Help System: PC-DMIS Fixturing (View Core Help)

#### List of Global Settings for Manual Machines

- Fixture Location: Path where you want that the fixture files (.ext.&.fxt ) be saved.

- Module Location: This specifies the full path of the location where modules will be saved.

- Status Location: Location where the fixture data file is saved.

- Standby Values for automatic standby:

- Create Standby Command(0/1)

- Optional Settings

- Standby Plane

- XY for vertical

- ZX for robots

- Common Axis convention:

- 0 = Convention for Horizontal CMM (default)

- 1 = Global with common axis