Current Help System: PC-DMIS Fixturing (View Core Help)

To Create a Custom CAD Model

1. Create a new part program.

2. Import the model via one of the standard PC-DMIS import options (i.e. IGES, STEP, etc.).

3. Save the part program. PC-DMIS creates a .CAD file with the same name as the part program in the same directory as the part program file.

4. Rename this file to anything you like.

5. Place this file in a directory of your choice to be used later.