Current Help System: PC-DMIS Laser (View Core Help)

#### Filter Type: Inline

This is only available for Metris sensors.

The Inline filter allows you to thin the data in the laser stripe. You specify the point Density along the stripe and the data returned to PC-DMIS will automatically be filtered according to the density specified.

Point Reduction Filter: This check box determines whether or not PC-DMIS filters points along the scan line. If marked, you can select the desired percentage of total points to filter. If cleared, the complete data set is acquired without any filtering.

Example of Point Filtering Disabled

Example of Point Filtering of 50%