Current Help System: PC-DMIS NC (View Core Help)

### Data Flow Chart for PC-DMIS NC

In the chart below, the following process is described:

1. Create a PC-DMIS Part Program

2. Open the Part Program in PC-DMIS NC.

3. Select the Operation | Create CNC Program menu option. PC-DMIS NC creates the NC program file.

4. Start the PC-DMIS CNC Server program.

5. Click Analyze Hold.

6. Select Download NC Program button. The NC program file gets sent to the NC controller.

7. Click Analyze Run.

- The NC machine with probing capability measures the features by taking probing hits.

- The NC program execution results get sent to PC-DMIS CNC Server.

- The PC-DMIS NC Server generates a journal file for later analysis and review.

- PC-DMIS NC runs the analysis phase to generate measurement results.