Current Help System: PC-DMIS NC (View Core Help)

#### Scans

- Advanced Scans – Unsupported. A CAD model is required to generate scan paths since there is no interactive learning. The model is used to generate a move / measure point set which is downloaded to the CNC controller for execution or executed directly using PC-DMIS NCI.

- BASIC Scans – Unsupported. These are controller dependent for generating the scan data.

- Stitch Scanning - Supported when using predefined paths. Supported in PC-DMIS NCI for predefined or adaptive paths.

- Execute Mode – NORMAL only is supported. Relearn is not supported.

- Nominals – MASTER and FINDNOMS are supported.